**SmartLine® Controller Enclosure**

**SLWMM**

POWDER-COATED STEEL ENCLOSURES shall be model SLWM-M-1600 or SLWM-M-4800 as manufactured by Weathermatic Sprinkler Division of Telsco Industries.

CONSTRUCTION: Enclosures shall be fabricated from 16 gauge powder-coated steel. Enclosures shall be NEMA type 3R rated weather-resistant. A removable powder-coated steel door shall be mounted to the front of the enclosure and include a cam style key-lock to restrict access to the enclosure.

SLWM-M-1600 Enclosure shall measure 13 ¼” wide x 14 ¼” high x 6 ¼” deep.

SLWM-M-4800 Enclosure shall measure 19 ½” wide x 19 ½” high x 7 ¾” deep.

WARRANTY: Enclosures shall have a manufacturer’s limited warranty of two (2) years.