**Powder-Coated Steel Enclosure
SLPED-ENC-M-4800 / SLPED-ENC-M-1600**

POWDER-COATED STEEL PEDESTAL ENCLOSURE shall be model SLPED-ENC-M-4800 or SLPED-ENC-M-1600 as manufactured by Weathermatic Sprinkler Division of Telsco Industries

CONSTRUCTION: Pedestal enclosure shall be fabricated from 16-gauge steel with a powder-coated finish. The enclosure shall be NEMA type 3R rated weather-resistant with filtered side louvers for cross-ventilation. A removable stainless steel door shall be mounted to the front of the enclosure and include a cam style key-lock to restrict access to the enclosure.

The cabinet shall be fabricated from 16-gauge steel with a powder-coated finish. The cabinet shall be NEMA type 3R rated weather-resistant. A removable stainless steel door shall be mounted to the front of the cabinet and include a cam style key-lock to restrict access to the cabinet.

SLPED-ENC-M-1600 Enclosure shall measure 13 ¼” wide x 44 ¼” high x 6 ¼” deep.

SLPED-ENC-M-4800 Enclosure shall measure 19 ½” wide x 44 ¼” high x 7 ¾” deep.

WARRANTY: Enclosure shall have a manufacturer’s limited warranty of two (2) years.