IRRIGATION

1. PRODUCTS
	* + 1. QUICK COUPLING VALVE
				1. QUICK COUPLING VALVE(s) shall be No. 7600 Series Valves as manufactured by Weathermatic Sprinkler Division of Telsco Industries, or approved equal.

Valve shall be made of rod brass and shall have a permanently attached spring retracted rubber cover.

For models 7644 and 7645 the cover shall be molded in the standard purple color of reclaimed water and include a molded-in warning. The warning shall be in Spanish and English and illustrated by the international symbol.

Valves shall use Acme® threads allowing gradual opening and closing.

The valve shall be capable of handling 1/2" to 1" bearing impact sprinklers and deliver up to 20 GPM at 125 psi.

The valve shall have a replaceable retainer nut and the seal shall be of rubber.

Inlet threads shall be one inch (FIP).

* + - * 1. The valve shall have a manufacturer’s over the counter exchange warranty of not less than five (5) years.